[Program]
Id=AVRDUDESHELL
Help=adshelpeng.chm
Language=E&nglish

[Language]
RandomEeprom=&Randomize EEPROM memory
RandomFlash=&Randomize FLASH memory
CreateRandomEeprom=&Create random EEPROM memory?
CreateRandomFlash=&Create random FLASH memory?
AVRDUDEconfig=&AVRDUDE config...
Report=&Report...
Copy=&Copy
Savedialog1=Any file (*.*)|*.*|BAT-file (*.bat)|*.bat
Savedialog2=Any file (*.*)|*.*|FLASH (*.hex)|*.hex|EEPROM (*.eep)|*.eep|Fuses (*.fus)|*.fus
Opendialog2=Any file (*.*)|*.*|FLASH (*.hex)|*.hex|EEPROM (*.eep)|*.eep|Fuses (*.fus)|*.fus
ErrorConnectToInternet1=&Information about updates could not be received because of internet disconnection. Check connection settings, proxy settings or try again later.
NoUpdate=&You are using the latest version. Updates no available now.
CheckUpdate=Check &updates...
UpdateProgram=Program updating
NewVers=&Your version of program is outdated. Last changes list is below. Please, visit the home page and download the update.
NewVersAvailable=&New version of program is available
HomePage=&Go to site for update
Free=free
SelectAll=Select all
UnSelectAll=Select none
Ok=O&k
Action=&Action
Cancel=&Cancel
Close=&Close
File=&File
Edit=&Edit
View=&View
Chip=&Chip
Property=&Properties
Help=&Help
New=&New
Open=&Open...
SaveAs=&Save as...
Disasm=Disasse&mbler
SaveProject=&Save all
Exit=&Exit
Reopen=&Open last
Find=&Find...
FindNext=Find &next
Header=&Header...
Delete=&Delete?
FindText=&Find text
CaseSensitive=Case &insensitive
TextOrHexData=&Text or HEX data to search:
Toolbar=&Toolbar
Statusbar=Status &bar
ComandLine=&Command line
ÑompactView=&Compact view
AdditionalInformation=&Additional info
FuseDefault=&Load fuse bits settings
FuseDefaultSet=&Save fuse bits settings
FuseInfo=Fuse bits &info...
SaveFuse=Save fuse
EnterFuseName=E&nter name for save fuses and press "Ok" button.
FuseNameExists=Settings exists. Enter other name.
SelectFuse=Select fuse data and press "Ok" button.
Read=&Read...
Write=&Write
Clear=&Clear...
AsCMD=As &CMD
All=&All...
Add=&Add
Fuse=&Fuse bits
Flash=&FLASH
Eeprom=&EEPROM
Chip=&Chip
MaxAddressWidth=Addres to max width
Programmer=&Programmer
Settings=&Settings...
GlossaryAndIndexes=&Contents and index
About=&About
Find=Find...
FindNext=Find next
ReadEEPROM=Read &EEPROM...
ReadFLASH=Read &FLASH...
ReadFuse=Read &fuse bits...
WriteEEPROM=Write &EEPROM...
WriteFLASH=Write &FLASH...
WriteFuse=Write &fuse bits...
FlashDesc=&FLASH - Program memory
EepromDesc=&EEPROM - Data memory
ChipNoSelect=&Chip not select
ChipNoSupport=&Chip not supported
SPIblocked=Blocking of programming by SPI
NoSelProg=Not checked - means "programmed"
SelProg=Checked - means "programmed"
NoFount=&Not found.
UserStoped=&Aborted by user.
FileNoFount=File &is missing.
ClearChip=&Erase chip?
APIError=&WinAPI error.
ProgrammerNoSupport=Programmer not &supported.
ProgrammerNoConnect=Programmer not &connected.
ChipNoCorrect=&Chip not as expected.
SignatureError=&Signature reading error.
ChipNoResponse=&Chip not response.
RAMNoSelect=&Memory type not specified.
ProjectNoSave=Project not saved. Save it?
FUSENotSave=FUSES not saved. Save it?
FLASHNotSave=FLASH not saved. Save it?
EEPROMNotSave=EEPROM not saved. Save it?
HEXChecksumError=&Checksum error in hex file. If this error will be repeated, please, contact the developer.
BufferError=&Error when assigning buffer.
ParamError=&Error parsing parameters
FileFormatError=&Incorrect file format.
DeleteCache=&Clear cache?
FileNoSupport=&Filetype not supported.
AVRDUDENoFount=&AVRDUDE not found in specified folder.
ErrorRAMSize=&Memory size mismatch an expected value.
DelayProgError=Incorrect value of &delay before bit sending.
SPIblockedAlert=Chip will be &locked for SPI programming. Continue anyway?
ErrorSizeFound=Incorrect &size of data to search.
ErrorGetSupporChip=&Error getting supported MCUs list. Check program folders: "Settings - Properties - Files and Folders".
ErrorGetSupporProgrammer=&Error getting supported programmers list. Check program folders: "Settings - Properties - Files and Folders".
LoadError=&Error loading file.
Source=&Source:
ErrorParseFuse=&Unable parsing the information on the specified fuse bits. If this error will be repeated, please, contact the developer.
ConnectToInternet=&Connecting to the internet and receive data...
ErrorConnectToInternet=&Information about programmed fuse bits could not be received because of internet disconnection. Check connection settings, proxy settings or try again later.
ReView=&Browse...
ReloadProgram=&The program needs to be restarted
NoName=No name
Property100=&General
Property101=&General program settings.
Property102=&Watch changes if project files
Property103=&Minimize to system tray
Property104=Global hotkey to write &FLASH(Ctrl+Q)
Property105=Global hotkey to write &EEPROM (Ctrl+E)
Property106=Global hotkey to write &fuse bits (Ctrl+T)
Property107=&Invert fuse bits checkboxes
Property108=Automatically set &fuse bits to default
Property109=Check &updates (weekly)
Property110=Auto load proj&ect file
Property111=Register ext (*.hex, *.eep, *.fus) for programm
Property200=&Files and Folders
Property201=&For normal program run, please, specify necessary files and folders.
Property202=&Default text editor for header file editing:
Property203=&Folder contain *.inc files with chip parameters. Header files is compatible with *.inc files of AVRStudio:
Property204=&AVRDUDE folder:
Property301=&There is a possibility to receive additional info about programmed fuse bits from site http://www.engbedded.com/ before programming.
Property302=&Show additional info
Property303=Enable &caching the result
Property400=&Proxy
Property401=&There is a possibility to use proxy for internet connection.
Property402=&Use proxy server
Property403=&User:
Property404=&Password:
Property405=&Port:
Property406=&Sever:
Property407=&Basic authentication
Property500=&Signature
Property501=&By default, AVRDUDE check chip signature before every programming. Sometimes signature of microcontroller damaged (erased or overwrited), but microcontroller  continues to function properly.
Property502=&Disable signature checking
Property600=&Counter
Property601=&Specify AVRDUDE to use last four bytes EEPROM memory to track how many times this microcontroller was erased/writed.
Property602=&Enable chip erase/wtite counter
Property700=&Port
Property701=&Specify port is connected to the programmer, for example LPT1, COM1, FT0.
Property800=&Additionally
Property801=&Additional parameters, which may be required on launch avrdude set here.
Property901=&For a bitbang programmers, make delay in microseconds before each sending every bit. If your  PC too fast or MCU works on too low frequency (from 32 KHz chrystal or internal 128 KHz RC generator), setting this option allows comply with the condition on which the ISP frequency should not exceed 1/4 MCU's clock.
Property1001=&Redefine RS-232 connection speed, specified for programmer in config file.
Property1101=&Specify bit clock period for JTAG interface or ISP clock (for JTAG ICE only). Value – number of microseconds. By default, JTAG ICE uses bit clock period equal 1 microsecond, suitable for microcontrollers which worked on 4 MHz frequency and above.
Property1201=&Disable automatically erasing of FLASH and EEPROM memory before programming. Automatically erasing of flash not used for ATxmega MCUs.
Property1202=&Disable automatically erasing
Property1301=&By default, AVRDUDE return parallel port in same state, which was before programming. This option change state of RESET and Vcc lines of parallel port  according to the arguments:
Property1302=&On RESET line will be leave low level, for leave microcontroller if RESET state.
Property1303=&On RESET line will be set high level, for microcontroller start up after programming.
Property1304=&This option set low level on "Vcc" line after programming.
Property1305=&This option set high level on "Vcc" line, which can be used to microcontroller powering.
Property1401=&AVRDUDE configuration
Property1501=&If to include this parameter special assembly of the avrdude program for programming of chips through FTDI (FT232RL) will be used, and some opportunities of the program will be blocked
Property1502=&Enable FTDI
lowsign=&LOW
lowname=&LOW fuse bits
lowdescription=The &low fuse byte
highsign=&HIGH
highname=&HIGH fuse bits
highdescription=The &high fuse byte
extendedsign=&EXTENDED
extendedname=&EXTENDED fuse bits
extendeddescription=The &extended fuse byte
calibrationsign=&CALIBRATION
calibrationname=&CALIBRATION data
calibrationdescription=Bytes of &RC oscillator calibration data
eepromsign=&EEPROM
eepromname=&EEPROM
eepromdescription=The &EEPROM of the device
flashsign=&FLASH
flashname=&FLASH
flashdescription=The &flash ROM of the device
fusesign=&FUSE
fusename=Single &fuse byte
fusedescription=The &fuse byte in devices that have only a single fuse byte
locksign=&LOCK
lockname=&Lock byte
lockdescription=The &lock byte
signaturesign=&SIGNATURE
signaturename=&Signature bytes
signaturedescription=Three device &signature bytes (device ID)
erasesign=&ERASE
erasename=FLASH and EEPROM memory &erase
erasedescription=FLASH and EEPROM memory &erase
SelectMemForRead=Select memory for reading 
SelectMemForWrite=Select memory for writing 
SelectMemForReadAlt=Specify memory for &reading 
SelectMemForWriteAlt=Specify memory for &writing
SelectMem=&Memory select
HintI=Enable microseconds delay|before each bit sending
HintB=Redefine RS-232 connection speed
HintBB=Use bit clock period|for JTAG or ISP clock
HintD=Disable automatically erasing|FLASH and EEPROM memory
HintER=Change state of|RESET line of parallel port
HintEV=Change state of|Vcc line of parallel port
HintF=Disable signature checking
HintY=Enable chip erase/write counter
HintP=Use specified port
HintW=Enable other parameters

